
1. Input AT+ATED to make the A11 enter RF test mode.
2. Click and run RT5350QA, connect the Ethernet port of module to computer(Need to Enable module Ethernet function by AT+FEPHY first). Then click OK of the following picture.



1. According to the following picture to adjust the RF parameter.

